00000000000i[     ] Bochs x86 Emulator 2.4.5
00000000000i[     ]   Build from CVS snapshot, on April 25, 2010
00000000000i[     ] System configuration
00000000000i[     ]   processors: 1 (cores=1, HT threads=1)
00000000000i[     ]   A20 line support: yes
00000000000i[     ] CPU configuration
00000000000i[     ]   level: 6
00000000000i[     ]   SMP support: no
00000000000i[     ]   APIC support: yes
00000000000i[     ]   FPU support: yes
00000000000i[     ]   MMX support: yes
00000000000i[     ]   3dnow! support: no
00000000000i[     ]   SEP support: yes
00000000000i[     ]   SSE support: sse2
00000000000i[     ]   XSAVE support: no
00000000000i[     ]   AES support: no
00000000000i[     ]   MOVBE support: no
00000000000i[     ]   x86-64 support: yes
00000000000i[     ]   1G paging support: no
00000000000i[     ]   MWAIT support: no
00000000000i[     ]   VMX support: no
00000000000i[     ] Optimization configuration
00000000000i[     ]   RepeatSpeedups support: yes
00000000000i[     ]   Trace cache support: yes
00000000000i[     ]   Fast function calls: yes
00000000000i[     ] Devices configuration
00000000000i[     ]   ACPI support: yes
00000000000i[     ]   NE2000 support: yes
00000000000i[     ]   PCI support: yes, enabled=yes
00000000000i[     ]   SB16 support: yes
00000000000i[     ]   USB support: yes
00000000000i[     ]   VGA extension support: vbe cirrus
00000000000i[MEM0 ] allocated memory at 03390020. after alignment, vector=03391000
00000000000i[MEM0 ] 32.00MB
00000000000i[MEM0 ] mem block size = 0x00100000, blocks=32
00000000000i[MEM0 ] rom at 0xfffe0000/131072 ('BIOS-bochs-latest')
00000000000i[MEM0 ] rom at 0xc0000/40448 ('VGABIOS-lgpl-latest')
00000000000i[CMOS ] Using local time for initial clock
00000000000i[CMOS ] Setting initial clock to: Mon Aug 30 16:24:59 2010 (time0=1283199899)
00000000000i[DMA  ] channel 4 used by cascade
00000000000i[DMA  ] channel 2 used by Floppy Drive
00000000000i[PCI  ] 440FX Host bridge present at device 0, function 0
00000000000i[PCI  ] PIIX3 PCI-to-ISA bridge present at device 1, function 0
00000000000i[MEM0 ] Register memory access handlers: 0x000a0000 - 0x000bffff
00000000000i[WGUI ] Desktop Window dimensions: 2048 x 1152
00000000000i[WGUI ] Number of Mouse Buttons = 4
00000000000i[WGUI ] IME disabled
00000000000i[MEM0 ] Register memory access handlers: 0xe0000000 - 0xe0ffffff
00000000000i[CLVGA] VBE Bochs Display Extension Enabled
00000000000i[CLVGA] interval=50000
00000000000i[     ] init_dev of 'unmapped' plugin device by virtual method
00000000000i[     ] init_dev of 'biosdev' plugin device by virtual method
00000000000i[     ] init_dev of 'speaker' plugin device by virtual method
00000000000i[     ] init_dev of 'extfpuirq' plugin device by virtual method
00000000000i[     ] init_dev of 'gameport' plugin device by virtual method
00000000000i[     ] init_dev of 'iodebug' plugin device by virtual method
00000000000i[     ] init_dev of 'pci_ide' plugin device by virtual method
00000000000i[PCI  ] PIIX3 PCI IDE controller present at device 1, function 1
00000000000i[     ] init_dev of 'acpi' plugin device by virtual method
00000000000i[PCI  ] ACPI Controller present at device 1, function 3
00000000000i[     ] init_dev of 'ioapic' plugin device by virtual method
00000000000i[IOAP ] initializing I/O APIC
00000000000i[MEM0 ] Register memory access handlers: 0xfec00000 - 0xfec00fff
00000000000i[     ] init_dev of 'keyboard' plugin device by virtual method
00000000000i[KBD  ] will paste characters every 1000 keyboard ticks
00000000000i[     ] init_dev of 'harddrv' plugin device by virtual method
00000000000i[HD   ] CD on ata0-0: 'M:\source\Cosmos\source2\Users\Kudzu\Breakpoints\bin\Debug\Breakpoints.iso'
00000000000i[CD1  ] load cdrom with path=M:\source\Cosmos\source2\Users\Kudzu\Breakpoints\bin\Debug\Breakpoints.iso
00000000000i[CD1  ] Opening image file as a cd
00000000000i[HD   ] Media present in CD-ROM drive
00000000000i[HD   ] Capacity is 1245 sectors (2.43 MB)
00000000000i[HD   ] Using boot sequence cdrom, none, none
00000000000i[HD   ] Floppy boot signature check is enabled
00000000000i[     ] init_dev of 'serial' plugin device by virtual method
00000000000i[SER  ] com1 at 0x03f8 irq 4
00000000000i[     ] init_dev of 'parallel' plugin device by virtual method
00000000000i[PAR  ] parallel port 1 at 0x0378 irq 7
00000000000i[     ] register state of 'unmapped' plugin device by virtual method
00000000000i[     ] register state of 'biosdev' plugin device by virtual method
00000000000i[     ] register state of 'speaker' plugin device by virtual method
00000000000i[     ] register state of 'extfpuirq' plugin device by virtual method
00000000000i[     ] register state of 'gameport' plugin device by virtual method
00000000000i[     ] register state of 'iodebug' plugin device by virtual method
00000000000i[     ] register state of 'pci_ide' plugin device by virtual method
00000000000i[     ] register state of 'acpi' plugin device by virtual method
00000000000i[     ] register state of 'ioapic' plugin device by virtual method
00000000000i[     ] register state of 'keyboard' plugin device by virtual method
00000000000i[     ] register state of 'harddrv' plugin device by virtual method
00000000000i[     ] register state of 'serial' plugin device by virtual method
00000000000i[     ] register state of 'parallel' plugin device by virtual method
00000000000i[SYS  ] bx_pc_system_c::Reset(HARDWARE) called
00000000000i[CPU0 ] cpu hardware reset
00000000000i[APIC0] allocate APIC id=0 (MMIO enabled) to 0xfee00000
00000000000i[CPU0 ] CPUID[0x00000000]: 00000003 756e6547 6c65746e 49656e69
00000000000i[CPU0 ] CPUID[0x00000001]: 00000f20 00000800 00002000 078bfbff
00000000000i[CPU0 ] CPUID[0x00000002]: 00410601 00000000 00000000 00000000
00000000000i[CPU0 ] CPUID[0x00000003]: 00000000 00000000 00000000 00000000
00000000000i[CPU0 ] CPUID[0x00000004]: 00000000 00000000 00000000 00000000
00000000000i[CPU0 ] CPUID[0x80000000]: 80000008 00000000 00000000 00000000
00000000000i[CPU0 ] CPUID[0x80000001]: 00000000 00000000 00000101 2a100800
00000000000i[CPU0 ] CPUID[0x80000002]: 20202020 20202020 20202020 6e492020
00000000000i[CPU0 ] CPUID[0x80000003]: 286c6574 50202952 69746e65 52286d75
00000000000i[CPU0 ] CPUID[0x80000004]: 20342029 20555043 20202020 00202020
00000000000i[CPU0 ] CPUID[0x80000006]: 00000000 42004200 02008140 00000000
00000000000i[CPU0 ] CPUID[0x80000007]: 00000000 00000000 00000000 00000000
00000000000i[CPU0 ] CPUID[0x80000008]: 00003020 00000000 00000000 00000000
00000000000i[     ] reset of 'unmapped' plugin device by virtual method
00000000000i[     ] reset of 'biosdev' plugin device by virtual method
00000000000i[     ] reset of 'speaker' plugin device by virtual method
00000000000i[     ] reset of 'extfpuirq' plugin device by virtual method
00000000000i[     ] reset of 'gameport' plugin device by virtual method
00000000000i[     ] reset of 'iodebug' plugin device by virtual method
00000000000i[     ] reset of 'pci_ide' plugin device by virtual method
00000000000i[     ] reset of 'acpi' plugin device by virtual method
00000000000i[     ] reset of 'ioapic' plugin device by virtual method
00000000000i[     ] reset of 'keyboard' plugin device by virtual method
00000000000i[     ] reset of 'harddrv' plugin device by virtual method
00000000000i[     ] reset of 'serial' plugin device by virtual method
00000000000i[     ] reset of 'parallel' plugin device by virtual method
00000000000i[     ] set SIGINT handler to bx_debug_ctrlc_handler
00000003305i[BIOS ] $Revision: 1.247 $ $Date: 2010/04/04 19:33:50 $
00000200000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00000318042i[KBD  ] reset-disable command received
00000444800i[VBIOS] VGABios $Id: vgabios.c,v 1.69 2009/04/07 18:18:20 vruppert Exp $

00000444871i[CLVGA] VBE known Display Interface b0c0
00000444903i[CLVGA] VBE known Display Interface b0c5
00000447828i[VBIOS] VBE Bios $Id: vbe.c,v 1.62 2009/01/25 15:46:25 vruppert Exp $
00000760517i[BIOS ] Starting rombios32
00000761014i[BIOS ] Shutdown flag 0
00000761695i[BIOS ] ram_size=0x02000000
00000762173i[BIOS ] ram_end=32MB
00000802745i[BIOS ] Found 1 cpu(s)
00000822014i[BIOS ] bios_table_addr: 0x000fbc18 end=0x000fcc00
00000822117i[PCI  ] 440FX PMC write to PAM register 59 (TLB Flush)
00001149814i[PCI  ] 440FX PMC write to PAM register 59 (TLB Flush)
00001477742i[P2I  ] PCI IRQ routing: PIRQA# set to 0x0b
00001477763i[P2I  ] PCI IRQ routing: PIRQB# set to 0x09
00001477784i[P2I  ] PCI IRQ routing: PIRQC# set to 0x0b
00001477805i[P2I  ] PCI IRQ routing: PIRQD# set to 0x09
00001477815i[P2I  ] write: ELCR2 = 0x0a
00001478700i[BIOS ] PIIX3/PIIX4 init: elcr=00 0a
00001486658i[BIOS ] PCI: bus=0 devfn=0x00: vendor_id=0x8086 device_id=0x1237 class=0x0600
00001489220i[BIOS ] PCI: bus=0 devfn=0x08: vendor_id=0x8086 device_id=0x7000 class=0x0601
00001491621i[BIOS ] PCI: bus=0 devfn=0x09: vendor_id=0x8086 device_id=0x7010 class=0x0101
00001491851i[PIDE ] new BM-DMA address: 0xc000
00001492555i[BIOS ] region 4: 0x0000c000
00001494865i[BIOS ] PCI: bus=0 devfn=0x0b: vendor_id=0x8086 device_id=0x7113 class=0x0680
00001495103i[ACPI ] new irq line = 11
00001495117i[ACPI ] new irq line = 9
00001495147i[ACPI ] new PM base address: 0xb000
00001495161i[ACPI ] new SM base address: 0xb100
00001495189i[PCI  ] setting SMRAM control register to 0x4a
00001659283i[CPU0 ] Enter to System Management Mode
00001659293i[CPU0 ] RSM: Resuming from System Management Mode
00001823313i[PCI  ] setting SMRAM control register to 0x0a
00001832484i[BIOS ] MP table addr=0x000fbcf0 MPC table addr=0x000fbc20 size=0xd0
00001834543i[BIOS ] SMBIOS table addr=0x000fbd00
00001836931i[BIOS ] ACPI tables: RSDP addr=0x000fbe20 ACPI DATA addr=0x01ff0000 size=0x988
00001840169i[BIOS ] Firmware waking vector 0x1ff00cc
00001851282i[PCI  ] 440FX PMC write to PAM register 59 (TLB Flush)
00001852126i[BIOS ] bios_table_cur_addr: 0x000fbe44
00005733768i[BIOS ] IDE time out
00017845409i[BIOS ] Booting from 07c0:0000
00023874830i[SER  ] com1: FIFO enabled
